**User Guide to Live Video**

1. Connect camera to Desktop windows computer. Run Cam Manager.exe


2. Use Cam Manager to set up WiFi and 4G information.

1) Enter default password 000000 and connect device

2) Turn on 4G and click Apply button.

3) Turn on Wi-Fi and click Apply button

4）Enter Wi-Fi SSID, password, Server IP and Apply.




If you are using our server, the server IP is 18.193.78.55

**Live Streaming Software Setting**


1. Download and install CMSV client software for windows. You can install APK for Android or search CMSV in Apple Store for IOS version.

Downloading Link:


<http://18.193.78.55:88/808gps/login.html?1629771756596>



1. After installation, open CMSV client and enter account, password and server IP to login into the system.



1. After login, check if camera is online. If the color of person icon is green, the camera obtained GPS signal. If it is Grey, the camera did not obtain GPS signal. You may need to go outside for better GPS signal.



1. If the camera is not online, please check if your WiFi SSID and Server information correct. **Also make sure your Device ID is same and correct as what you set on CMSV Server.**

